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Job Safety Analysis
Task-based risk assessment
	Complete this with the workers doing the task, at the work area, before work starts. If the task is high-risk construction work, a safe work method statement (SWMS) is also required.



1. Task details
	Task
What is being done
	

	Site / project
	
	Location on site
	

	Company
	
	Supervisor
	

	JSA number
	
	Date
	

	Related SWMS (if any)
	
	Permits required
	



2. Site conditions checked at the work area
	☐  Ground stable and level
	☐  Weather suitable
	☐  Overhead powerlines or services

	☐  Underground services located
	☐  Access and egress clear
	☐  Other trades working nearby

	☐  Public or traffic interface
	☐  Lighting adequate
	☐  Housekeeping and trip hazards

	☐  Edges, openings and penetrations
	☐  Hazardous materials present
	☐  Noise or dust from other work

	☐  Other: ____________________
	
	



3. Risk rating
Rate each step before and after controls.
	Likelihood ↓ / Consequence →
	Insignificant
	Minor
	Moderate
	Major
	Catastrophic

	Almost certain
	M
	H
	H
	E
	E

	Likely
	M
	M
	H
	H
	E

	Possible
	L
	M
	H
	H
	E

	Unlikely
	L
	L
	M
	H
	H

	Rare
	L
	L
	M
	M
	H


 E   Extreme: do not start. Eliminate or redesign the task before any work.
 H   High: work only with higher-order controls in place and a supervisor sign-off.
 M   Medium: controls in place, monitored during the task.
 L   Low: manage by routine procedures.

4. Steps, hazards and controls
	Step
	Hazards
	Risk before
	Controls
	Risk after
	Who

	EXAMPLE  Carry gutter lengths from stack to scaffold
	Manual handling of long lengths; trip hazards on the path
	M
	Two-person carry for lengths over one person's reach; clear and mark the carry path first; gloves for sharp edges.
	L
	Both installers

	EXAMPLE  Fix gutter brackets from the scaffold
	Fall from height; dropped tools onto path below
	H
	Scaffold with full edge protection and tag current; tool lanyards; exclusion zone below with barrier.
	M
	Leading hand

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	



5. Protective equipment for this task
	☐  Hard hat
	☐  Safety glasses
	☐  Hi-vis
	☐  Safety boots

	☐  Gloves
	☐  Hearing protection
	☐  Respirator
	☐  Harness

	☐  Face shield
	☐  Sun protection
	☐  Knee pads
	☐  Long clothing

	☐  Other: ____________________
	
	
	



6. Stop-work triggers
	Stop and reassess if: the weather changes, the method or equipment changes, another trade starts work in the area, a control cannot be put in place, or anyone feels unsafe. Update this JSA and re-brief before restarting.



7. Crew sign-on
I helped prepare or was briefed on this JSA, I understand it and I will follow it.
	Name
	Company
	Role
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



8. Supervisor review
	Reviewed by
	
	Date
	

	Changes made during the task
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