
	pointCPD
	Plant pre-start checklist
Doc no. ________   Revision ____   Date ____________


Plant pre-start checklist
Daily check for mobile plant
	Complete before first use each shift. Follow the manufacturer's operator manual for this machine as well. If any item marked with a safety fault fails, tag the machine out of service and report it. Do not operate faulty plant.



1. Machine and operator
	Plant type
Excavator, skid steer, EWP, telehandler, forklift, roller
	
	Make and model
	

	ID / registration / hire number
	
	Hour meter reading
	

	Operator
	
	Licence / competency
High risk work licence where required
	

	Site
	
	Week starting
	



2. Walk-around and fluids (engine off)
	#
	Check
	Mon
	Tue
	Wed
	Thu
	Fri
	Sat
	Sun

	1
	No fluid leaks under or around the machine
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	2
	Engine oil level
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	3
	Coolant level
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	4
	Hydraulic oil level
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	5
	Fuel level and cap secure
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	6
	Tyres (pressure, damage) or tracks (tension, damage)
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	7
	Hydraulic hoses and fittings: no leaks, chafing or damage
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	8
	Bucket, attachment, pins and teeth secure
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	9
	Quick hitch: safety pin or lock in place and working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	10
	Guards, covers and steps in place
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	11
	Lights, beacon and reflectors clean and intact
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	12
	Mirrors and windows clean and undamaged
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	13
	Operator manual and load chart in the cab
	☐
	☐
	☐
	☐
	☐
	☐
	☐



3. Cab and safety devices
	#
	Check
	Mon
	Tue
	Wed
	Thu
	Fri
	Sat
	Sun

	1
	Seat and seat belt in good condition and working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	2
	ROPS / FOPS structure undamaged
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	3
	Horn working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	4
	Reversing alarm working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	5
	Camera or proximity system working (if fitted)
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	6
	Fire extinguisher present and in date
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	7
	Emergency stop working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	8
	EWP: harness anchor, gate, emergency lowering and tilt alarm working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	9
	Forklift or telehandler: forks, chains and load backrest in good condition
	☐
	☐
	☐
	☐
	☐
	☐
	☐



4. Start-up and function test (in a clear area)
	#
	Check
	Mon
	Tue
	Wed
	Thu
	Fri
	Sat
	Sun

	1
	No warning lights or abnormal gauge readings
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	2
	Service and park brakes working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	3
	Steering working correctly
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	4
	All hydraulic functions smooth and responsive
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	5
	Quick hitch locks correctly under test
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	6
	Slew, travel and boom functions working (as applicable)
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	7
	Isolation or lock-out working
	☐
	☐
	☐
	☐
	☐
	☐
	☐

	8
	No unusual noises, smoke or vibration
	☐
	☐
	☐
	☐
	☐
	☐
	☐



5. Daily sign-off
	Day
	Result
	Operator signature
	Supervisor sighted

	EXAMPLE  Mon
	OK to operate
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



6. Faults and repairs
	Date
	Fault
	Safety fault? (tagged out)
	Reported to
	Repaired by / date
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