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Site safety inspection checklist
Weekly workplace inspection for building sites
	Tick Yes if the item is in place and satisfactory, No if it needs action (record it in section 9), N/A if it does not apply to the current stage.



1. Inspection details
	Site / project
	
	Date
	

	Inspected by
	
	Accompanied by
	

	Current stage of work
	
	Trades on site today
	



2. Site security, access and signage
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Perimeter fencing secure, no gaps, gates lockable
	☐
	☐
	☐
	

	2
	Site sign with principal contractor name and after-hours contact
	☐
	☐
	☐
	

	3
	Safety signage at entry (PPE, induction, visitor sign-in)
	☐
	☐
	☐
	

	4
	Sign-in register in use
	☐
	☐
	☐
	

	5
	Safe pedestrian access separate from vehicles
	☐
	☐
	☐
	

	6
	Delivery and set-down areas defined, not on edges or paths
	☐
	☐
	☐
	

	7
	Footpath and road kept clear; any permit conditions met
	☐
	☐
	☐
	

	8
	Neighbouring properties protected (runoff, debris, overhang)
	☐
	☐
	☐
	



3. Working at heights
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Edge protection in place on slab edges, roofs, balconies, stairs and voids
	☐
	☐
	☐
	

	2
	Floor openings and penetrations covered, secured and marked
	☐
	☐
	☐
	

	3
	Scaffold tagged, tag current, inspected within the required period
	☐
	☐
	☐
	

	4
	Scaffold complete: guardrails, mid-rails, toe boards, access, no missing planks
	☐
	☐
	☐
	

	5
	Only competent people altering scaffold
	☐
	☐
	☐
	

	6
	Ladders in good condition, correct type, set up and secured properly
	☐
	☐
	☐
	

	7
	Mobile scaffolds and platforms on level ground, wheels locked
	☐
	☐
	☐
	

	8
	Harness and anchor systems inspected and used where required
	☐
	☐
	☐
	

	9
	Exclusion zones below overhead work
	☐
	☐
	☐
	



4. Plant and equipment
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Pre-start checks completed and recorded for mobile plant
	☐
	☐
	☐
	

	2
	Operators hold required licences
	☐
	☐
	☐
	

	3
	Exclusion zones and spotters for mobile plant
	☐
	☐
	☐
	

	4
	Reversing alarms and lights working
	☐
	☐
	☐
	

	5
	Guards fitted to saws, grinders and other power tools
	☐
	☐
	☐
	

	6
	Registered plant documents on site where required
	☐
	☐
	☐
	

	7
	Lifting gear inspected and tagged
	☐
	☐
	☐
	

	8
	Plant kept clear of overhead powerlines
	☐
	☐
	☐
	



5. Electrical
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Temporary switchboard secured, weatherproof and labelled
	☐
	☐
	☐
	

	2
	Residual current devices in use and tested
	☐
	☐
	☐
	

	3
	Leads and tools tested and tagged, tags current
	☐
	☐
	☐
	

	4
	Leads elevated off the ground and out of water and traffic
	☐
	☐
	☐
	

	5
	No damaged leads, plugs or double adaptors
	☐
	☐
	☐
	

	6
	Overhead and underground services identified and marked
	☐
	☐
	☐
	



6. Excavations and ground
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Underground services located before digging (Before You Dig Australia)
	☐
	☐
	☐
	

	2
	Excavations protected: shoring, benching or battering as designed
	☐
	☐
	☐
	

	3
	Spoil and materials kept back from edges
	☐
	☐
	☐
	

	4
	Barriers and signage around excavations
	☐
	☐
	☐
	

	5
	Safe access and egress from trenches
	☐
	☐
	☐
	

	6
	Excavations inspected after rain or ground movement
	☐
	☐
	☐
	



7. Health, hazardous materials and housekeeping
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Dust controlled at the source when cutting (extraction, water, score-and-snap)
	☐
	☐
	☐
	

	2
	Respiratory protection available and worn where required
	☐
	☐
	☐
	

	3
	Asbestos register sighted for existing buildings; suspect material left alone
	☐
	☐
	☐
	

	4
	Hazardous chemicals stored correctly with current safety data sheets
	☐
	☐
	☐
	

	5
	Hearing protection used for noisy work
	☐
	☐
	☐
	

	6
	Heat and sun: shade, water and rest breaks available
	☐
	☐
	☐
	

	7
	Walkways and work areas clear of rubbish and offcuts
	☐
	☐
	☐
	

	8
	Nails, reo and sharp edges capped or removed
	☐
	☐
	☐
	

	9
	Waste bins not overfull; waste separated
	☐
	☐
	☐
	

	10
	Materials stacked stably and within safe heights
	☐
	☐
	☐
	

	11
	Adequate lighting for work areas and access
	☐
	☐
	☐
	



8. First aid, emergency and amenities
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	First aid kit stocked and accessible
	☐
	☐
	☐
	

	2
	Trained first aider identified
	☐
	☐
	☐
	

	3
	Emergency plan and contact numbers displayed
	☐
	☐
	☐
	

	4
	Fire extinguishers in date and accessible, especially near hot work
	☐
	☐
	☐
	

	5
	Assembly point signed
	☐
	☐
	☐
	

	6
	Toilets clean and serviced
	☐
	☐
	☐
	

	7
	Drinking water available
	☐
	☐
	☐
	

	8
	Meal area and hand-washing available
	☐
	☐
	☐
	

	9
	SWMS on site for all current high-risk work
	☐
	☐
	☐
	

	10
	Induction records current for everyone on site
	☐
	☐
	☐
	



9. Actions required
	Item #
	Issue found
	Action
	Risk
	Owner
	Due
	Closed

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	



10. Sign-off
	Inspector signature
	
	Date
	

	Actions from last inspection closed?
	
	Next inspection due
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