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Waterproofing inspection checklist
Internal wet areas and external balconies: before covering
	Inspect after the membrane has cured and before any screed, bedding or tiles are laid. Check against AS 3740 (internal wet areas), the external waterproofing requirements for balconies and decks, and the membrane manufacturer's instructions. One checklist per wet area.



1. Area and system
	Site
	
	Area
Ensuite, bathroom, laundry, WC, balcony
	

	Membrane product and system
	
	Membrane type
Liquid, sheet; under or over screed
	

	Waterproofer
	
	Licence number
	

	Date applied
	
	Curing time per manufacturer
	



2. Substrate, falls and drainage
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Substrate clean, dry, sound and cured before membrane applied
	☐
	☐
	☐
	

	2
	Substrate type compatible with the membrane system
	☐
	☐
	☐
	

	3
	Primer applied as the manufacturer requires
	☐
	☐
	☐
	

	4
	Floor falls to the waste as designed, no ponding
	☐
	☐
	☐
	

	5
	Shower area set-down or hob as designed
	☐
	☐
	☐
	

	6
	Puddle flanges fitted and sealed into the membrane
	☐
	☐
	☐
	

	7
	Waste outlets at the correct height
	☐
	☐
	☐
	

	8
	Balcony: falls away from the building, outlets and overflow provided
	☐
	☐
	☐
	

	9
	Balcony: threshold height or step-down as designed
	☐
	☐
	☐
	



3. Membrane extent and application
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Floor fully waterproofed where required for the area
	☐
	☐
	☐
	

	2
	Shower area walls waterproofed to the required height and width
	☐
	☐
	☐
	

	3
	Walls outside the shower treated as required (splash zones, wall-floor junction)
	☐
	☐
	☐
	

	4
	Bath and spa surrounds treated as required
	☐
	☐
	☐
	

	5
	Membrane continuous with consistent colour and coverage
	☐
	☐
	☐
	

	6
	Applied at the manufacturer's thickness (wet film or coats as specified)
	☐
	☐
	☐
	

	7
	No pinholes, blisters, thin spots or damage
	☐
	☐
	☐
	

	8
	Reinforcing fabric installed where the system requires it
	☐
	☐
	☐
	



4. Junctions and penetrations
	#
	Check
	Yes
	No
	N/A
	Comments / action

	1
	Bond breakers or flexible sealant at wall-floor and wall-wall junctions
	☐
	☐
	☐
	

	2
	Internal and external corners reinforced as the system requires
	☐
	☐
	☐
	

	3
	Membrane overlaps at junctions as required
	☐
	☐
	☐
	

	4
	Water stop angle at the shower or wet area perimeter and door threshold
	☐
	☐
	☐
	

	5
	Membrane lapped onto water stops and puddle flanges
	☐
	☐
	☐
	

	6
	Pipe penetrations sealed with collars or flanges
	☐
	☐
	☐
	

	7
	Tap and mixer penetrations sealed
	☐
	☐
	☐
	

	8
	Balcony: membrane turned up behind door sill and under cladding as detailed
	☐
	☐
	☐
	



5. Flood test and evidence
	Flood test done?
Where specified
	
	Duration and result
	

	Checked below for leaks by
	
	Photos of every junction taken?
	

	Waterproofer's certificate received (date)
	
	Certifier inspection (if required)
	



6. Defects and rectification
	Location
	Defect
	Action
	Re-checked (date)

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



7. Released for tiling
	Inspected by
	
	Signature
	

	Date
	
	Tiler told membrane must not be damaged
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